Ascom Nexion

Next Hop Resolution Protocol

Version 8-Beta

Presented By: James V. Luciani

AscomNexion

Next Hop Resolution ProtocolVersion 8-Beta

James V. Luciani

n Changes for NHRPv8-Beta

q A multitude of wording changes. q A don’t reply bit has been added to the NHRP Purge Request. q I used the term LAG somewhat in error in v7. q The NHRP Resolution Reply now has a NAK Code ¥ There may be more than one reason for a NAK to be sent, and there were a number of folks interested in differentiating the reasons. This replaces the "P" bit.

q Two error codes have been re-included

¥6 - Protocol Address Unreachable : Can�t get there from here along routed path ¥7 - Protocol Error: E.g., packet format error q Added the error code for failed authentication in the NHRP Error Indication ¥11 - Authentication Failure

AscomNexion

Next Hop Resolution ProtocolVersion 8-Beta

James V. Luciani

n Still unanswered questions:

q Do we want an error indication to be sent when the hop count is exceeded?

q Should NHRP Registration Replies be routed by NBMA address or by Protocol Address?